**The normal cross section of NSM laminates**

50mm

The width of laminate is 50mm.

Thickness of laminate is 1.4 mm.

**Cutting of NSM laminates**

Laminate strips

Table1. Size and quantity of laminate strips after cutting

|  |  |  |
| --- | --- | --- |
| SI.NO | Size of Laminate strips (after cutting) (mm) | Quantity (No.s) |
| 1 | 12.5\*1.4\*900 | 176 |
| 2 | 12.5\*1.4\*450 | 16 |
| 3 | 12.5\*1.4\*1350 | 16 |
| 4 | 12.5\*1.4\*1800 | 16 |
| 5 | 14.06\*1.4\*900 | 32 |
| Total | | 256 |