1. Man power assistance for removing air bags from the roughness tester machine.
2. Fixing of air leakage within air bags
3. Re arranging the set up for its original condition.
4. Calibration for surface flatness.